!
! pimd sample configuration file
!
hostname quagga-pimd-router
password zebra
!enable password zebra
!
!log file pimd.log
log stdout
!
line vty
 exec-timeout 60
!
!debug igmp
!debug pim
!debug pim zebra
!
ip multicast-routing
!
! ! You may want to enable ssmpingd for troubleshooting
! ! See http://www.venaas.no/multicast/ssmping/
! !
! ip ssmpingd 1.1.1.1
! ip ssmpingd 2.2.2.2
!
! ! HINTS:
! !  - Enable "ip pim ssm" on the interface directly attached to the
! !    multicast source host (if this is the first-hop router)
! !  - Enable "ip pim ssm" on pim-routers-facing interfaces
! !  - Enable "ip igmp" on IGMPv3-hosts-facing interfaces
! !  - In order to inject IGMPv3 local membership information in the
! !    PIM protocol state, enable both "ip pim ssm" and "ip igmp" on
! !    the same interface; otherwise PIM won't advertise
! !    IGMPv3-learned membership to other PIM routers
!
interface eth0
 ip pim ssm
 ip igmp

! -x-
